# $Id$
# Used by Example.yard
#
# inittab	This file describes how the INIT process should set up
#		the system in a certain run-level.
#
# Version:	@(#)inittab		2.04	17/05/93	MvS
#                                       2.10    02/10/95        PV
#                                       3.00    02/06/1999      PV
#
# Author:	Miquel van Smoorenburg, <miquels@drinkel.nl.mugnet.org>
# Modified by:	Patrick J. Volkerding, <volkerdi@ftp.cdrom.com>
#

# These are the default runlevels in Slackware:
#   0 = halt
#   1 = single user mode
#   2 = unused (but configured the same as runlevel 3)
#   3 = multiuser mode (default Slackware runlevel)
#   4 = X11 with KDM/GDM/XDM (session managers)
#   5 = unused (but configured the same as runlevel 3)
#   6 = reboot

# Default runlevel. (Do not set to 0 or 6)
id:3:initdefault:

# System initialization (runs when system boots).
si:S:sysinit:/etc/init.d/rcS

# Script to run when going single user (runlevel 1).
su:1S:wait:/sbin/sulogin

# Script to run when going multi user.
rc:2345:wait:/etc/init.d/rc

# What to do at the "Three Finger Salute".
ca::ctrlaltdel:/sbin/shutdown -t5 -rf now

# Runlevel 0 halts the system.
l0:0:wait:/etc/init.d/halt

# Runlevel 6 reboots the system.
l6:6:wait:/etc/init.d/reboot

# What to do when power fails (shutdown to single user).
pf::powerfail:/sbin/shutdown -f +5 "THE POWER IS FAILING"

# If power is back before shutdown, cancel the running shutdown.
pg:0123456:powerokwait:/sbin/shutdown -c "THE POWER IS BACK"

# If power comes back in single user mode, return to multi user mode.
ps:S:powerokwait:/sbin/init 3

# The getties in multi user mode on consoles an serial lines.
#
# NOTE NOTE NOTE adjust this to your getty or you will not be
#                able to login !!
#
# Note: for 'agetty' you use linespeed, line.
# for 'getty_ps' you use line, linespeed and also use 'gettydefs'
c1:1235:respawn:/sbin/agetty 38400 ttys/0 linux
c2:1235:respawn:/sbin/agetty 38400 ttys/1 linux
c3:1235:respawn:/sbin/agetty 38400 ttys/2 linux
#c4:1235:respawn:/sbin/agetty 38400 tty4 linux
#c5:1235:respawn:/sbin/agetty 38400 tty5 linux
#c6:12345:respawn:/sbin/agetty 38400 tty6 linux

# Serial lines
#s1:12345:respawn:/sbin/agetty 19200 ttyS0 vt100
#s2:12345:respawn:/sbin/agetty 19200 ttyS1 vt100

# Dialup lines
#d1:12345:respawn:/sbin/agetty -mt60 38400,19200,9600,2400,1200 ttyS0 vt100
#d2:12345:respawn:/sbin/agetty -mt60 38400,19200,9600,2400,1200 ttyS1 vt100

# Runlevel 4 used to be for an X window only system, until we discovered
# that it throws init into a loop that keeps your load avg at least 1 all 
# the time. Thus, there is now one getty opened on tty6. Hopefully no one
# will notice. ;^)
# It might not be bad to have one text console anyway, in case something 
# happens to X.
# x1:4:wait:/etc/rc.d/rc.4

# End of /etc/inittab



