# /etc/network/interfaces -- configuration file for ifup(8), ifdown(8)
#
# $Id$
# make_debian replacement

# The loopback interface
auto lo
iface lo inet loopback

# You will want to edit this for your requirements.

# In the example below the host was set-up in this way:
# ifconfig tap0 192.168.1.5
# route add -host 192.168.1.4 gw 192.168.1.5 

#auto eth0
#iface eth0 inet static
#	address 192.168.1.2
#	netmask 255.255.255.0
#	network 192.168.1.0
#	broadcast 192.168.1.255
#	gateway 192.168.1.5
