$Id$
make_debian-X11 replacement

Setting up the root filesystem
-----------------------------

1. Run setup in this directory: 

. setup

Setting up a Swap File
----------------------

1. Run make_swapfile in this directory:

. make_swapfile


Getting X working
-----------------

1. To get X11 working you will need to get your network up.  The instructions
below assume your host (the computer you are running) has an ip of 192.168.1.4,
a uml ip of 192.168.1.2 and a tap device ip of 192.168.1.5.

2. If you haven't already done this, you will want to edit the 
/etc/network/interfaces file using vi.  This should be self-explanatory.

3. Load any modules required by your host system.  If you decide to use 
tap, do this: 

modprobe ethertap
modprobe netlink_dev

4. Configure the device on your host system.  Here the tap device is being
set to 192.168.1.5 and then routed to the host 192.168.1.4:

ifconfig tap0 192.168.1.5
route add -host 192.168.1.4 gw 192.168.1.5

5. The next time you start the uml kernel and boot the root_fs you will want 
to give it options like this where  HWaddr (see ifconfig) belongs to your 
network device:

ubd0=/root_fs_debian_x11 root=/dev/ubd0 eth0=ethertap,tap0,HWaddr,192.168.1.5 mem=64M

Hint: An easier way to do this would be to use the UML box in gbootroot from
your host computer.  No ..  uml doesn't work within uml. :)

6. At this point you should be able to ping 192.168.1.4.

Hint: Check to make sure that uml_net came bundled with the uml kernel,
because this is what enables networking.

6.  Run startx.  It will ask for your host ip number.

That's it.  

Links:
user-mode-linux.sourceforge.net

Hints:
Mount the host fs:  mount -t hostfs none /mnt
		    mount -t hostfs none -o /home /mnt

Jonathan Rosenbaum
freeesource@users.sourceforge.net


